LSPNL4MIB DEFINITIONS ::= BEGIN

--
-- Top-level infrastructure of the Net-SNMP project enterprise MIB tree
--

IMPORTS
    MODULE-IDENTITY, enterprises          	FROM SNMPv2-SMI
    MODULE-IDENTITY, OBJECT-TYPE, Integer32,
    NOTIFICATION-TYPE                       FROM SNMPv2-SMI
    SnmpAdminString                         FROM SNMP-FRAMEWORK-MIB
    netSnmp                                 FROM NET-SNMP-MIB
    RowStatus, StorageType, DisplayString   FROM SNMPv2-TC
    InetAddressType, InetAddress            FROM INET-ADDRESS-MIB
;
LSPNL4MIB MODULE-IDENTITY
    LAST-UPDATED "202103041010Z"
    ORGANIZATION "LifeSafety Power, Inc. "
    CONTACT-INFO    
     "http://www.lifesafetypower.com/
	 
	  EMail: gliu@lifesafetypower.com
	 "
    DESCRIPTION
    "This is the MIB Module for NL4 and NL2 objects for managing NL4/NL2 device."

	REVISION	"202103041010Z"
	DESCRIPTION
	"Updated to support Net-SNMP compile."
    ::= { enterprises 42520}
    


NL4MIB OBJECT IDENTIFIER ::= {LSPNL4MIB 3}  




fp1         	OBJECT IDENTIFIER ::= { NL4MIB 1}
fp2        		OBJECT IDENTIFIER ::= { NL4MIB 2}
nac1        	OBJECT IDENTIFIER ::= { NL4MIB 4}
nac2         	OBJECT IDENTIFIER ::= { NL4MIB 5}
m8-1          	OBJECT IDENTIFIER ::= { NL4MIB 7}
m8-1-1  		OBJECT IDENTIFIER ::= { m8-1  1}
m8-1-2  		OBJECT IDENTIFIER ::= { m8-1  2}
m8-1-3  		OBJECT IDENTIFIER ::= { m8-1  3}
m8-1-4  		OBJECT IDENTIFIER ::= { m8-1  4}
m8-1-5  		OBJECT IDENTIFIER ::= { m8-1  5}
m8-1-6  		OBJECT IDENTIFIER ::= { m8-1  6}
m8-1-7  		OBJECT IDENTIFIER ::= { m8-1  7}
m8-1-8  		OBJECT IDENTIFIER ::= { m8-1  8}
m8-2          	OBJECT IDENTIFIER ::= { NL4MIB 8}
m8-2-1  		OBJECT IDENTIFIER ::= { m8-2  1}
m8-2-2  		OBJECT IDENTIFIER ::= { m8-2  2}
m8-2-3  		OBJECT IDENTIFIER ::= { m8-2  3}
m8-2-4  		OBJECT IDENTIFIER ::= { m8-2  4}
m8-2-5  		OBJECT IDENTIFIER ::= { m8-2  5}
m8-2-6  		OBJECT IDENTIFIER ::= { m8-2  6}
m8-2-7  		OBJECT IDENTIFIER ::= { m8-2  7}
m8-2-8  		OBJECT IDENTIFIER ::= { m8-2  8}
m8-3          	OBJECT IDENTIFIER ::= { NL4MIB 9}
m8-3-1  		OBJECT IDENTIFIER ::= { m8-3  1}
m8-3-2  		OBJECT IDENTIFIER ::= { m8-3  2}
m8-3-3  		OBJECT IDENTIFIER ::= { m8-3  3}
m8-3-4  		OBJECT IDENTIFIER ::= { m8-3  4}
m8-3-5  		OBJECT IDENTIFIER ::= { m8-3  5}
m8-3-6  		OBJECT IDENTIFIER ::= { m8-3  6}
m8-3-7  		OBJECT IDENTIFIER ::= { m8-3  7}
m8-3-8  		OBJECT IDENTIFIER ::= { m8-3  8}
netlink       	OBJECT IDENTIFIER ::= { NL4MIB 10}
sd16-1          	OBJECT IDENTIFIER ::= { NL4MIB 16}
sd16-1-1  		OBJECT IDENTIFIER ::= { sd16-1  1}
sd16-1-2  		OBJECT IDENTIFIER ::= { sd16-1  2}
sd16-1-3  		OBJECT IDENTIFIER ::= { sd16-1  3}
sd16-1-4  		OBJECT IDENTIFIER ::= { sd16-1  4}
sd16-1-5  		OBJECT IDENTIFIER ::= { sd16-1  5}
sd16-1-6  		OBJECT IDENTIFIER ::= { sd16-1  6}
sd16-1-7  		OBJECT IDENTIFIER ::= { sd16-1  7}
sd16-1-8  		OBJECT IDENTIFIER ::= { sd16-1  8}
sd16-1-9  		OBJECT IDENTIFIER ::= { sd16-1  9}
sd16-1-10  		OBJECT IDENTIFIER ::= { sd16-1  10}
sd16-1-11  		OBJECT IDENTIFIER ::= { sd16-1  11}
sd16-1-12  		OBJECT IDENTIFIER ::= { sd16-1  12}
sd16-1-13  		OBJECT IDENTIFIER ::= { sd16-1  13}
sd16-1-14  		OBJECT IDENTIFIER ::= { sd16-1  14}
sd16-1-15  		OBJECT IDENTIFIER ::= { sd16-1  15}
sd16-1-16  		OBJECT IDENTIFIER ::= { sd16-1  16}
sd16-2          	OBJECT IDENTIFIER ::= { NL4MIB 17}
sd16-2-1  		OBJECT IDENTIFIER ::= { sd16-2  1}
sd16-2-2  		OBJECT IDENTIFIER ::= { sd16-2  2}
sd16-2-3  		OBJECT IDENTIFIER ::= { sd16-2  3}
sd16-2-4  		OBJECT IDENTIFIER ::= { sd16-2  4}
sd16-2-5  		OBJECT IDENTIFIER ::= { sd16-2  5}
sd16-2-6  		OBJECT IDENTIFIER ::= { sd16-2  6}
sd16-2-7  		OBJECT IDENTIFIER ::= { sd16-2  7}
sd16-2-8  		OBJECT IDENTIFIER ::= { sd16-2  8}
sd16-2-9  		OBJECT IDENTIFIER ::= { sd16-2  9}
sd16-2-10  		OBJECT IDENTIFIER ::= { sd16-2  10}
sd16-2-11  		OBJECT IDENTIFIER ::= { sd16-2  11}
sd16-2-12  		OBJECT IDENTIFIER ::= { sd16-2  12}
sd16-2-13  		OBJECT IDENTIFIER ::= { sd16-2  13}
sd16-2-14  		OBJECT IDENTIFIER ::= { sd16-2  14}
sd16-2-15  		OBJECT IDENTIFIER ::= { sd16-2  15}
sd16-2-16  		OBJECT IDENTIFIER ::= { sd16-2  16}
sd16-3          	OBJECT IDENTIFIER ::= { NL4MIB 18}
sd16-3-1  		OBJECT IDENTIFIER ::= { sd16-3  1}
sd16-3-2  		OBJECT IDENTIFIER ::= { sd16-3  2}
sd16-3-3  		OBJECT IDENTIFIER ::= { sd16-3  3}
sd16-3-4  		OBJECT IDENTIFIER ::= { sd16-3  4}
sd16-3-5  		OBJECT IDENTIFIER ::= { sd16-3  5}
sd16-3-6  		OBJECT IDENTIFIER ::= { sd16-3  6}
sd16-3-7  		OBJECT IDENTIFIER ::= { sd16-3  7}
sd16-3-8  		OBJECT IDENTIFIER ::= { sd16-3  8}
sd16-3-9  		OBJECT IDENTIFIER ::= { sd16-3  9}
sd16-3-10  		OBJECT IDENTIFIER ::= { sd16-3  10}
sd16-3-11  		OBJECT IDENTIFIER ::= { sd16-3  11}
sd16-3-12  		OBJECT IDENTIFIER ::= { sd16-3  12}
sd16-3-13  		OBJECT IDENTIFIER ::= { sd16-3  13}
sd16-3-14  		OBJECT IDENTIFIER ::= { sd16-3  14}
sd16-3-15  		OBJECT IDENTIFIER ::= { sd16-3  15}
sd16-3-16  		OBJECT IDENTIFIER ::= { sd16-3  16}

NL4Traps       	OBJECT IDENTIFIER ::= { LSPNL4MIB 4}




--
--	FP1
--    
FP1Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Time."
    DEFVAL { "" }
    ::= { fp1  1 }

FP1DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FPO ID."
    DEFVAL { "" }
    ::= { fp1  2 }

FP1ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply Model, Such as FPO75-25, FPO150-100, FPO250-200."
    DEFVAL { "" }
    ::= { fp1  3 }

FP1SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply system fault status."
    DEFVAL { "" }
    ::= { fp1  4 }

FP1ACFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply AC lost status, No or Yes."
    DEFVAL { "" }
    ::= { fp1  5 }

FP1FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI status."
    DEFVAL { "" }
    ::= { fp1  6 }

FP1OutputLatchingOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI latch status."
    DEFVAL { "" }
    ::= { fp1  7 }
    
FP1ACInputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC input voltage."
    DEFVAL { "" }
    ::= { fp1  8 }

FP1OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output voltage."
    DEFVAL { "" }
    ::= { fp1  9 }
    
FP1OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output Current."
    DEFVAL { "" }
    ::= { fp1  10 }
    

FP1BatteryVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System battery voltage."
    DEFVAL { "" }
    ::= { fp1  11 }

FP1BatteryChargeCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery charge current."
    DEFVAL { "" }
    ::= { fp1  12 }
    
FP1BatteryFaultDetect OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery Fault Detect. For AQL/FPV."
    DEFVAL { "" }
    ::= { fp1  13 }

FP1TotalPowerupTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power supply total runtime."
    DEFVAL { "" }
    ::= { fp1  14 }

FP1BatteryInstalledTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery install hours."
    DEFVAL { "" }
    ::= { fp1  15 }

FP1NumberOfACFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC lost count."
    DEFVAL { "" }
    ::= { fp1  16 }

FP1NumberOfSystemFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System fault count."
    DEFVAL { "" }
    ::= { fp1  17 }
	
	
FP1RatedBatteryLife OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "FPO battery lifetime."
    DEFVAL { "" }
    ::= { fp1  18 }	

	
FP1RatedCapacity  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery capacity."
    DEFVAL { "" }
    ::= { fp1  19 }	
	
		
FP1BatteryStateOfCharge OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "The FPO battery state of charge."
    DEFVAL { "" }
    ::= { fp1  20 }	


FP1BatteryStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable calculate battery state of charge."
    DEFVAL { "" }
    ::= { fp1  21 }		
		
FP1BatteryTestStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery discharge test status, Active or Inactive"
    DEFVAL { "" }
    ::= { fp1  22 }

FP1BatteryLastTestDate OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test date."
    DEFVAL { "" }
    ::= { fp1  23 }

FP1BatteryLastTestDischargeTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test time."
    DEFVAL { "" }
    ::= { fp1  24 }
    
FP1RepeatTestInterval OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Repeat Test Interval."
    DEFVAL { "" }
    ::= { fp1  25 }
    
FP1Version	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FP1 Ver."
    DEFVAL { "" }
    ::= { fp1  26 }  
    
FP1SystemFaultDescription	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Fault Description."
    DEFVAL { "" }
    ::= { fp1  27 }         
    
 FP1BatteryTestsPerformed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Performed."
    DEFVAL { "" }
    ::= { fp1  28 }   

FP1BatteryTestsFailed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Failed."
    DEFVAL { "" }
    ::= { fp1  29 }  

   FP1RequiredBatteryRuntime	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS   read-write
    STATUS      current
    DESCRIPTION
    "Required Battery Runtime."
    DEFVAL { "" }
    ::= { fp1  30 }  

    FP1ActualStandby	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Actual Standby."
    DEFVAL { "" }
    ::= { fp1  31 }  

    FP1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset output for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { fp1  32 }  

    FP1BatteryScheduleTestDateTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "e.g. Enter '2020-01-01 23:01:59' to configure Battery Schedule Test DateTime"
    DEFVAL { "" }
    ::= { fp1  33 }  

   FP1OutputResetDelay OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Output Reset Delay Seconds for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { fp1  34 }  
  

--
--	FP2
--    
FP2Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { fp2  1 }

FP2DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { fp2  2 }

FP2ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { fp2  3 }
FP2SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply system fault status."
    DEFVAL { "" }
    ::= { fp2  4 }

FP2ACFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply AC lost status, No or Yes."
    DEFVAL { "" }
    ::= { fp2  5 }

FP2FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI status."
    DEFVAL { "" }
    ::= { fp2  6 }

FP2OutputLatchingOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI latch status."
    DEFVAL { "" }
    ::= { fp2  7 }
    
FP2ACInputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC input voltage."
    DEFVAL { "" }
    ::= { fp2  8 }

FP2OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output voltage."
    DEFVAL { "" }
    ::= { fp2  9 }
    
FP2OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output Current."
    DEFVAL { "" }
    ::= { fp2  10 }
    

FP2BatteryVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System battery voltage."
    DEFVAL { "" }
    ::= { fp2  11 }

FP2BatteryChargeCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery charge current."
    DEFVAL { "" }
    ::= { fp2  12 }
    
FP2BatteryFaultDetect OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery Fault Detect. For AQL/FPV."
    DEFVAL { "" }
    ::= { fp2  13 }

FP2TotalPowerupTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power supply total runtime."
    DEFVAL { "" }
    ::= { fp2  14 }

FP2BatteryInstalledTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery install hours."
    DEFVAL { "" }
    ::= { fp2  15 }

FP2NumberOfACFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC lost count."
    DEFVAL { "" }
    ::= { fp2  16 }

FP2NumberOfSystemFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System fault count."
    DEFVAL { "" }
    ::= { fp2  17 }
	
	
FP2RatedBatteryLife OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "FPO battery lifetime."
    DEFVAL { "" }
    ::= { fp2  18 }	

	
FP2RatedCapacity  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery capacity."
    DEFVAL { "" }
    ::= { fp2  19 }	
	
		
FP2BatteryStateOfCharge OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "The FPO battery state of charge."
    DEFVAL { "" }
    ::= { fp2  20 }	


FP2BatteryStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable calculate battery state of charge."
    DEFVAL { "" }
    ::= { fp2  21 }		
		
FP2BatteryTestStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery discharge test status, Active or Inactive"
    DEFVAL { "" }
    ::= { fp2  22 }

FP2BatteryLastTestDate OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test date."
    DEFVAL { "" }
    ::= { fp2  23 }

FP2BatteryLastTestDischargeTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test time."
    DEFVAL { "" }
    ::= { fp2  24 }
    
FP2RepeatTestInterval OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Repeat Test Interval."
    DEFVAL { "" }
    ::= { fp2  25 }
    
 FP2Version	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FP2 Ver."
    DEFVAL { "" }
    ::= { fp2  26 }  
    
FP2SystemFaultDescription	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Fault Description."
    DEFVAL { "" }
    ::= { fp2  27 }    
   
     FP2BatteryTestsPerformed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Performed."
    DEFVAL { "" }
    ::= { fp2  28 }   

FP2BatteryTestsFailed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Failed."
    DEFVAL { "" }
    ::= { fp2  29 }  

   FP2RequiredBatteryRuntime	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Required Battery Runtime."
    DEFVAL { "" }
    ::= { fp2  30 }  

    FP2ActualStandby	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Actual Standby."
    DEFVAL { "" }
    ::= { fp2  31 } 

    FP2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset output for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { fp2  32 }  

    FP2BatteryScheduleTestDateTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "e.g. Enter '2020-01-01 23:01:59' to configure Battery Schedule Test DateTime"
    DEFVAL { "" }
    ::= { fp2  33 }  

    FP2OutputResetDelay OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Output Reset Delay Seconds for AQL/FPV-G2/FPG/FPO-G2"
    DEFVAL { "" }
    ::= { fp2  34 }  

--
--	NAC1
--    
NAC1Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Time."
    DEFVAL { "" }
    ::= { nac1  1 }

NAC1DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "NAC device ID."
    DEFVAL { "" }
    ::= { nac1  2 }

NAC1ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Device model is N24,NULL for none device detected."
    DEFVAL { "" }
    ::= { nac1  3 }

NAC1SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Fault Status, No or Yes."
    DEFVAL { "" }
    ::= { nac1  4 }

NAC1FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI Status, Active or Inactive"
    DEFVAL { "" }
    ::= { nac1  5 }

NAC1ModeStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "NAC model, Supervisory or Alarm model."
    DEFVAL { "" }
    ::= { nac1  6 }
    
NAC1Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "NAC Ver."
    DEFVAL { "" }
    ::= { nac1  7 }    

--
--	NAC2
--    
NAC2Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nac2  1 }

NAC2DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nac2  2 }

NAC2ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nac2  3 }

NAC2SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nac2  4 }

NAC2FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nac2  5 }

NAC2ModeStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nac2  6 }
    
NAC2Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nac2  7 }    

		
--
--	m8-1
--    		

m8-1-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { m8-1-1  1 }

m8-1-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { m8-1-1  2 }

m8-1-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { m8-1-1  3 }

m8-1-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { m8-1-1  4 }
	
m8-1-1PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- power supply."
    DEFVAL { "" }
    ::= { m8-1-1  5 }	
	
	
m8-1-1ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- Output response to control input, Active, Inactive or Disable."
    DEFVAL { "" }
    ::= { m8-1-1  6 }		
	
m8-1-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { m8-1-1  7 }		
	
	
m8-1-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { m8-1-1  8 }

m8-1-1CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- control Input Type, Normally Open, Normally Closed,
    Open Collector, Voltage, Disabled."
    DEFVAL { "" }
    ::= { m8-1-1  9 }	
	
	
m8-1-1OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- output load type, Maglock, Fail-safe Strike, 
    Fail-secure Strike, Constant ON."
    DEFVAL { "" }
    ::= { m8-1-1  10 }	
	
m8-1-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on FAI Activation, Yes or No."
    DEFVAL { "" }
    ::= { m8-1-1  11 }	
	
	
m8-1-1UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on AC loss, Yes or No."
    DEFVAL { "" }
    ::= { m8-1-1  12 }	
	
m8-1-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { m8-1-1  13 }		
	
m8-1-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { m8-1-1  14 }		
	
m8-1-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { m8-1-1  15 }	
	
m8-1-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { m8-1-1  16 }	
	

m8-1-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { m8-1-1  17 }	

m8-1-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable M8 -."
    DEFVAL { "" }
    ::= { m8-1-1  18 }	

m8-1-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-1-1  19 }		
	
	
--
--	m8-1
--    



m8-1-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  1 }

m8-1-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  2 }

m8-1-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  3 }

m8-1-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  4 }
	
m8-1-2PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  5 }	
	
	
m8-1-2ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  6 }		
	
m8-1-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  7 }		
	
	
m8-1-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  8 }		

m8-1-2CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  9 }	
	
m8-1-2OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  10 }	

m8-1-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  11 }	
	
	
m8-1-2UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  12 }	
	
m8-1-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  13 }		
	
m8-1-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  14 }		
	
m8-1-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  15 }	
	
m8-1-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  16 }	
	

m8-1-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  17 }		

	
m8-1-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  18 }	

m8-1-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-1-2  19 }	
	
--
--	m8-1
--    
	

m8-1-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  1 }

m8-1-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  2 }

m8-1-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  3 }

m8-1-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  4 }
	
m8-1-3PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  5 }	
	
	
m8-1-3ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  6 }		
	
m8-1-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  7 }		
	
	
m8-1-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  8 }
	

m8-1-3CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  9 }


m8-1-3OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  10 }	
	

m8-1-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  11 }	
	
	
m8-1-3UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  12 }	
	
m8-1-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  13 }		
	
m8-1-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  14 }		
	
m8-1-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  15 }	
	
m8-1-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  16 }	
	

m8-1-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  17 }	


m8-1-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  18 }	

m8-1-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-1-3  19 }	
	
--
--	m8-1
--    
	
	

m8-1-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  1 }

m8-1-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  2 }

m8-1-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  3 }

m8-1-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  4 }
	
m8-1-4PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  5 }	
	
	
m8-1-4ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  6 }		
	
m8-1-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  7 }		
	
	
m8-1-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  8 }		
	

m8-1-4CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  9 }	
	

m8-1-4OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  10 }	


m8-1-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  11 }	
	
	
m8-1-4UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  12 }	
	
m8-1-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  13 }		
	
m8-1-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  14 }		
	
m8-1-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  15 }	
	
m8-1-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  16 }	
	

m8-1-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  17 }	

	
m8-1-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  18 }	

m8-1-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-1-4  19 }	

	
--
--	m8-1
--    

	
	

m8-1-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  1 }

m8-1-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  2 }

m8-1-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  3 }

m8-1-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  4 }
	
m8-1-5PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  5 }	
	
	
m8-1-5ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  6 }		
	
m8-1-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  7 }		
	
	
m8-1-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  8 }	
	

m8-1-5CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  9 }
	
	
m8-1-5OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  10 }	
	
	
m8-1-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  11 }	
	
	
m8-1-5UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  12 }	
	
m8-1-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  13 }		
	
m8-1-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  14 }		
	
m8-1-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  15 }	
	
m8-1-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  16 }	
	

m8-1-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  17 }	

m8-1-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  18 }	

m8-1-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-1-5  19 }		
	
--
--	m8-1
--    
	

m8-1-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  1 }

m8-1-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  2 }

m8-1-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  3 }

m8-1-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  4 }
	
m8-1-6PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  5 }	
	
	
m8-1-6ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  6 }		
	
m8-1-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  7 }		
	
	
m8-1-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  8 }	


m8-1-6CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  9 }

	
m8-1-6OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  10 }	
	
m8-1-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  11 }	
	
	
m8-1-6UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  12 }	
	
m8-1-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  13 }		
	
m8-1-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  14 }		
	
m8-1-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  15 }	
	
m8-1-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  16 }	
	

m8-1-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  17 }	

	
m8-1-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  18 }	

m8-1-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-1-6  19 }		
	
--
--	m8-1
--    

m8-1-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  1 }

m8-1-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  2 }

m8-1-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  3 }

m8-1-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  4 }
	
m8-1-7PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  5 }	
	
	
m8-1-7ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  6 }		
	
m8-1-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  7 }		
	
	
m8-1-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  8 }	


m8-1-7CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  9 }

m8-1-7OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  10 }	

m8-1-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  11 }	
	
	
m8-1-7UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  12 }	
	
m8-1-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  13 }		
	
m8-1-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  14 }		
	
m8-1-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  15 }	
	
m8-1-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  16 }	
	

m8-1-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  17 }		

m8-1-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  18 }	

m8-1-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-1-7  19 }		
	
--
--	m8-1
--    	

m8-1-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  1 }

m8-1-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  2 }

m8-1-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  3 }

m8-1-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  4 }
	
m8-1-8PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  5 }	
	
	
m8-1-8ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  6 }		
	
m8-1-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  7 }		
	
	
m8-1-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  8 }		
	
	
m8-1-8CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  9 }


m8-1-8OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  10 }	

m8-1-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  11 }	
	
	
m8-1-8UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  12 }	
	
m8-1-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  13 }		
	
m8-1-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  14 }		
	
m8-1-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  15 }	
	
m8-1-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  16 }	
	

m8-1-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  17 }		

m8-1-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  18 }	

m8-1-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-1-8  19 }		
	
m8-1Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1  9 }	
    
m8-1VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1  10 }

m8-1VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1  11 }

m8-1CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1  12 }

 m8-1CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1  13 }
    
m8-1Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1  14 }

--
--	M8-2
--    


m8-2-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  1 }

m8-2-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  2 }

m8-2-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  3 }

m8-2-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  4 }
	
m8-2-1PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  5 }	
	
	
m8-2-1ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  6 }		
	
m8-2-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  7 }		
	
	
m8-2-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  8 }		
	
	
m8-2-1CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  9 }	
	

m8-2-1OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  10 }	

m8-2-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  11 }	
	
	
m8-2-1UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  12 }	
	
m8-2-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  13 }		
	
m8-2-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  14 }		
	
m8-2-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  15 }	
	
m8-2-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  16 }	
	

m8-2-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  17 }		
	

m8-2-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  18 }	

m8-2-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-2-1  19 }		
	
	
--
--	M8-2
--    

m8-2-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  1 }

m8-2-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  2 }

m8-2-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  3 }

m8-2-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  4 }
	
m8-2-2PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  5 }	
	
	
m8-2-2ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  6 }		
	
m8-2-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  7 }		
	
	
m8-2-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  8 }		


m8-2-2CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  9 }		
	
m8-2-2OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  10 }	

m8-2-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  11 }	
	
	
m8-2-2UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  12 }	
	
m8-2-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  13 }		
	
m8-2-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  14 }		
	
m8-2-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  15 }	
	
m8-2-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  16 }	
	

m8-2-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  17 }		

m8-2-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  18 }		

m8-2-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-2-2  19 }		
	
--
--	M8-2
--    


m8-2-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  1 }

m8-2-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  2 }

m8-2-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  3 }

m8-2-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  4 }
	
m8-2-3PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  5 }	
	
	
m8-2-3ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  6 }		
	
m8-2-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  7 }		
	
	
m8-2-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  8 }		


m8-2-3CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  9 }	
	

m8-2-3OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  10 }	

m8-2-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  11 }	
	
	
m8-2-3UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  12 }	
	
m8-2-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  13 }		
	
m8-2-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  14 }		
	
m8-2-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  15 }	
	
m8-2-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  16 }	
	

m8-2-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  17 }	

	
m8-2-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  18 }	

m8-2-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-2-3  19 }			
	
--
--	M8-2
--    

	

m8-2-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  1 }

m8-2-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  2 }

m8-2-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  3 }

m8-2-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  4 }
	
m8-2-4PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  5 }	
	
	
m8-2-4ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  6 }		
	
m8-2-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  7 }		
	
	
m8-2-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  8 }		

	
m8-2-4CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  9 }


m8-2-4OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  10 }	

m8-2-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  11 }	
	
	
m8-2-4UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  12 }	
	
m8-2-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  13 }		
	
m8-2-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  14 }		
	
m8-2-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  15 }	
	
m8-2-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  16 }	
	

m8-2-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  17 }		


m8-2-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  18 }	

m8-2-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-2-4  19 }			
	
--
--	M8-2
--    	

m8-2-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  1 }

m8-2-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  2 }

m8-2-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  3 }

m8-2-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  4 }
	
m8-2-5PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  5 }	
	
	
m8-2-5ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  6 }		
	
m8-2-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  7 }		
	
	
m8-2-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  8 }	
	

m8-2-5CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  9 }
	
	
m8-2-5OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  10 }	

m8-2-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  11 }	
	
	
m8-2-5UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  12 }	
	
m8-2-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  13 }		
	
m8-2-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  14 }		
	
m8-2-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  15 }	
	
m8-2-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  16 }	
	

m8-2-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  17 }	

m8-2-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  18 }	

m8-2-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-2-5  19 }				
	
--
--	M8-2
--    

m8-2-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  1 }

m8-2-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  2 }

m8-2-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  3 }

m8-2-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  4 }
	
m8-2-6PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  5 }	
	
	
m8-2-6ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  6 }		
	
m8-2-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  7 }		
	
	
m8-2-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  8 }	


m8-2-6CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  9 }

	
m8-2-6OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  10 }	

m8-2-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  11 }	
	
	
m8-2-6UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  12 }	
	
m8-2-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  13 }		
	
m8-2-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  14 }		
	
m8-2-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  15 }	
	
m8-2-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  16 }	
	

m8-2-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  17 }	

m8-2-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  18 }	

m8-2-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-2-6  19 }				
	
--
--	M8-2
--    


m8-2-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  1 }

m8-2-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  2 }

m8-2-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  3 }

m8-2-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  4 }
	
m8-2-7PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  5 }	
	
	
m8-2-7ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  6 }		
	
m8-2-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  7 }		
	
	
m8-2-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  8 }	


m8-2-7CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  9 }

	
m8-2-7OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  10 }	

m8-2-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  11 }	
	
	
m8-2-7UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  12 }	
	
m8-2-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  13 }		
	
m8-2-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  14 }		
	
m8-2-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  15 }	
	
m8-2-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  16 }	
	

m8-2-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  17 }	

m8-2-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  18 }	

m8-2-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-2-7  19 }				
	
--
--	M8-2
--    	

m8-2-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  1 }

m8-2-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  2 }

m8-2-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  3 }

m8-2-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  4 }
	
m8-2-8PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  5 }	
	
	
m8-2-8ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  6 }		
	
m8-2-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  7 }		
	
	
m8-2-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  8 }		
	
	
m8-2-8CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  9 }


m8-2-8OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  10 }	

m8-2-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  11 }	
	
	
m8-2-8UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  12 }	
	
m8-2-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  13 }		
	
m8-2-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  14 }		
	
m8-2-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  15 }	
	
m8-2-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  16 }	
	

m8-2-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  17 }	

m8-2-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  18 }	

m8-2-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-2-8  19 }				
	
m8-2Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2  9 }
    
m8-2VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2  10 }

m8-2VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2  11 }

m8-2CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2  12 }

 m8-2CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2  13 }
    
    
m8-2Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2  14 }    
    


--
--	M8-3
--    


m8-3-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  1 }

m8-3-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  2 }

m8-3-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  3 }

m8-3-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  4 }
	
m8-3-1PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  5 }	
	
	
m8-3-1ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  6 }		
	
m8-3-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  7 }		
	
	
m8-3-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  8 }		
	
	
m8-3-1CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  9 }	
	

m8-3-1OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  10 }	

m8-3-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  11 }	
	
	
m8-3-1UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  12 }	
	
m8-3-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  13 }		
	
m8-3-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  14 }		
	
m8-3-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  15 }	
	
m8-3-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  16 }	
	

m8-3-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  17 }		

m8-3-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  18 }	

m8-3-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-3-1  19 }				
	
	
--
--	M8-3
--    	

m8-3-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  1 }

m8-3-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  2 }

m8-3-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  3 }

m8-3-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  4 }
	
m8-3-2PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  5 }	
	
	
m8-3-2ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  6 }		
	
m8-3-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  7 }		
	
	
m8-3-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  8 }		
	

m8-3-2CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  9 }	

m8-3-2OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  10 }	

m8-3-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  11 }	
	
	
m8-3-2UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  12 }	
	
m8-3-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  13 }		
	
m8-3-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  14 }		
	
m8-3-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  15 }	
	
m8-3-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  16 }	
	

m8-3-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  17 }		

m8-3-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  18 }	

m8-3-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-3-2  19 }	
	
	
--
--	M8-3
--    

m8-3-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  1 }

m8-3-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  2 }

m8-3-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  3 }

m8-3-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  4 }
	
m8-3-3PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  5 }	
	
	
m8-3-3ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  6 }		
	
m8-3-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  7 }		
	
	
m8-3-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  8 }		
	

m8-3-3CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  9 }	


m8-3-3OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  10 }	

m8-3-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  11 }	
	
	
m8-3-3UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  12 }	
	
m8-3-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  13 }		
	
m8-3-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  14 }		
	
m8-3-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  15 }	
	
m8-3-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  16 }	
	

m8-3-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  17 }	

m8-3-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  18 }	

m8-3-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-3-3  19 }	
	
--
--	M8-3
--    
	

m8-3-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  1 }

m8-3-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  2 }

m8-3-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  3 }

m8-3-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  4 }
	
m8-3-4PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  5 }	
	
	
m8-3-4ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  6 }		
	
m8-3-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  7 }		
	
	
m8-3-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  8 }		
	

m8-3-4CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  9 }	
	
m8-3-4OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  10 }	

m8-3-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  11 }	
	
	
m8-3-4UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  12 }	
	
m8-3-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  13 }		
	
m8-3-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  14 }		
	
m8-3-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  15 }	
	
m8-3-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  16 }	
	

m8-3-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  17 }		
	
m8-3-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  18 }	

m8-3-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-3-4  19 }	
		
	
--
--	M8-3
--    
	

m8-3-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  1 }

m8-3-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  2 }

m8-3-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  3 }

m8-3-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  4 }
	
m8-3-5PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  5 }	
	
	
m8-3-5ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  6 }		
	
m8-3-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  7 }		
	
	
m8-3-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  8 }	
	

m8-3-5CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  9 }	

	
m8-3-5OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  10 }	

m8-3-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  11 }	
	
	
m8-3-5UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  12 }	
	
m8-3-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  13 }		
	
m8-3-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  14 }		
	
m8-3-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  15 }	
	
m8-3-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  16 }	
	

m8-3-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  17 }	

m8-3-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  18 }	

m8-3-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-3-5  19 }	
		
	
--
--	M8-3
--    


m8-3-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  1 }

m8-3-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  2 }

m8-3-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  3 }

m8-3-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  4 }
	
m8-3-6PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  5 }	
	
	
m8-3-6ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  6 }		
	
m8-3-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  7 }		
	
	
m8-3-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  8 }	


m8-3-6CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  9 }	


m8-3-6OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  10 }	

m8-3-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  11 }	
	
	
m8-3-6UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  12 }	
	
m8-3-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  13 }		
	
m8-3-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  14 }		
	
m8-3-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  15 }	
	
m8-3-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  16 }	
	

m8-3-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  17 }	

m8-3-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  18 }	

m8-3-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-3-6  19 }	
			

--
--	M8-3
--    


m8-3-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  1 }

m8-3-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  2 }

m8-3-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  3 }

m8-3-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  4 }
	
m8-3-7PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  5 }	
	
	
m8-3-7ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  6 }		
	
m8-3-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  7 }		
	
	
m8-3-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  8 }	


m8-3-7CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  9 }	

m8-3-7OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  10 }	

m8-3-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  11 }	
	
	
m8-3-7UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  12 }	
	
m8-3-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  13 }		
	
m8-3-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  14 }		
	
m8-3-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  15 }	
	
m8-3-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  16 }	
	

m8-3-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  17 }	

m8-3-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  18 }	

m8-3-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-3-7  19 }	
		
	
--
--	M8-3
--    


m8-3-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  1 }

m8-3-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  2 }

m8-3-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  3 }

m8-3-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  4 }
	
m8-3-8PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  5 }	
	
	
m8-3-8ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  6 }		
	
m8-3-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  7 }		
	
	
m8-3-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  8 }	


m8-3-8CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  9 }	

m8-3-8OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  10 }	

m8-3-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  11 }	
	
	
m8-3-8UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  12 }	
	
m8-3-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  13 }		
	
m8-3-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  14 }		
	
m8-3-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  15 }	
	
m8-3-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  16 }	
	

m8-3-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  17 }	

m8-3-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  18 }	

m8-3-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset M8 channel output."
    DEFVAL { "" }
    ::= { m8-3-8  19 }	
	

m8-3Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3  9 }
    
m8-3VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3  10 }

m8-3VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3  11 }

m8-3CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3  12 }

m8-3CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3  13 }

m8-3Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3  14 }        
    
    

--
--	MCU
--    
Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Time."
    DEFVAL { "" }
    ::= { netlink  1 }

SiteID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Site ID, it is entered by user from GUI."
    DEFVAL { "" }
    ::= { netlink  2 }

CabinetInternalTemperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System temperature on PCB board."
    DEFVAL { "" }
    ::= { netlink  3 }
    
CurrentSense1  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "HallSensor 1 Current."
    DEFVAL { "" }
    ::= { netlink  4 }
   
CurrentSense2  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "HallSensor 2 Current."
    DEFVAL { "" }
    ::= { netlink  5 }
    
ExternalTemperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Enviroment temperature."
    DEFVAL { "" }
    ::= { netlink  6 }
    
ADC1Reading OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    " ADC1 Voltage."
    DEFVAL { "" }
    ::= { netlink  7 }
    
ADC2Reading OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "ADC2 Voltage."
    DEFVAL { "" }
    ::= { netlink  8 }
    
Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Event1 status, Active or Inactive."
    DEFVAL { "" }
    ::= { netlink  10 }
    

CNTRL1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "NL4 Fault pin output status, set as ON will output 
    low voltage, OFF will output high voltage."
    DEFVAL { "" }
    ::= { netlink  12 }

CNTRL2 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "NL4 EN_FAI pin status, set as ON will output 
    low voltage, OFF will output high voltage."
    DEFVAL { "" }
    ::= { netlink  13 }

DeviceDetectCnt OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System device detected."
    DEFVAL { "" }
    ::= { netlink  14 }

NextServicedue OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Service due, NO or Yes. Service date is entered by user from GUI."
    DEFVAL { "" }
    ::= { netlink  15 }
    
Status   OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "MCU  Current Status."
    DEFVAL { "" }
    ::= { netlink  16 }
    
Version  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "MCU  Version."
    DEFVAL { "" }
    ::= { netlink  17 }    

SystemVersion  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Version."
    DEFVAL { "" }
    ::= { netlink  18 }    

--
--	sd16-1
--    



sd16-1-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-1  1 }

sd16-1-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-1  2 }

sd16-1-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-1  3 }

sd16-1-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-1  4 }
	
	
sd16-1-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-1  5 }		
	
	
sd16-1-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-1  6 }		

	
sd16-1-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-1  7 }		
	
sd16-1-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-1  8 }		
	
sd16-1-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-1  9 }	
	
sd16-1-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-1  10 }	
	

sd16-1-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-1  11 }		

	
sd16-1-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-1  12 }	

sd16-1-1ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-1  13 }	

sd16-1-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-1  14 }	

	

--
--	sd16-1
--    



sd16-1-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-2  1 }

sd16-1-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-2  2 }

sd16-1-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-2  3 }

sd16-1-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-2  4 }
	
	
sd16-1-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-2  5 }		
	
	
sd16-1-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-2  6 }		

	
sd16-1-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-2  7 }		
	
sd16-1-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-2  8 }		
	
sd16-1-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-2  9 }	
	
sd16-1-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-2  10 }	
	

sd16-1-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-2  11 }		

	
sd16-1-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-2  12 }	

sd16-1-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-2  13 }	

sd16-1-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-2  14 }	

	
--
--	sd16-1
--    
	

sd16-1-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-3  1 }

sd16-1-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-3  2 }

sd16-1-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-3  3 }

sd16-1-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-3  4 }
	
	
sd16-1-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-3  5 }		
	
	
sd16-1-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-3  6 }
	
	
sd16-1-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-3  7 }		
	
sd16-1-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-3  8 }		
	
sd16-1-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-3  9 }	
	
sd16-1-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-3  10 }	
	

sd16-1-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-3  11 }	


sd16-1-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-3  12 }	

sd16-1-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-3  13 }	

sd16-1-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-3  14 }	

	
--
--	sd16-1
--    
	
	

sd16-1-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-4  1 }

sd16-1-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-4  2 }

sd16-1-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-4  3 }

sd16-1-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-4  4 }
	
	
sd16-1-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-4  5 }		
	
	
sd16-1-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-4  6 }		
	
	
sd16-1-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-4  7 }		
	
sd16-1-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-4  8 }		
	
sd16-1-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-4  9 }	
	
sd16-1-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-4  10 }	
	

sd16-1-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-4  11 }	

	
sd16-1-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-4  12 }	

sd16-1-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-4  13 }	

sd16-1-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-4  14 }	


	
--
--	sd16-1
--    

	
	

sd16-1-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-5  1 }

sd16-1-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-5  2 }

sd16-1-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-5  3 }

sd16-1-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-5  4 }
	
	
sd16-1-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-5  5 }		
	
	
sd16-1-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-5  6 }	
	
	
sd16-1-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-5  7 }		
	
sd16-1-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-5  8 }		
	
sd16-1-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-5  9 }	
	
sd16-1-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-5  10 }	
	

sd16-1-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-5  11 }	

sd16-1-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-5  12 }	

sd16-1-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-5  13 }		

sd16-1-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-5  14 }	

	
--
--	sd16-1
--    
	

sd16-1-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-6  1 }

sd16-1-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-6  2 }

sd16-1-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-6  3 }

sd16-1-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-6  4 }
	
	
sd16-1-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-6  5 }		
	
	
sd16-1-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-6  6 }	

	
sd16-1-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-6  7 }		
	
sd16-1-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-6  8 }		
	
sd16-1-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-6  9 }	
	
sd16-1-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-6  10 }	
	

sd16-1-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-6  11 }	

	
sd16-1-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-6  12 }	

sd16-1-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-6  13 }		

sd16-1-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-6  14 }	

	
--
--	sd16-1
--    

sd16-1-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-7  1 }

sd16-1-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-7  2 }

sd16-1-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-7  3 }

sd16-1-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-7  4 }
	
	
sd16-1-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-7  5 }		
	
	
sd16-1-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-7  6 }	


	
sd16-1-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-7  7 }		
	
sd16-1-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-7  8 }		
	
sd16-1-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-7  9 }	
	
sd16-1-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-7  10 }	
	

sd16-1-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-7  11 }		

sd16-1-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-7  12 }	

sd16-1-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-7  13 }	

sd16-1-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-7  14 }	
	
	
--
--	sd16-1
--    	

sd16-1-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-8  1 }

sd16-1-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-8  2 }

sd16-1-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-8  3 }

sd16-1-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-8  4 }
	
	
sd16-1-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-8  5 }		
	
	
sd16-1-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-8  6 }		
	
	
	
sd16-1-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-8  7 }		
	
sd16-1-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-8  8 }		
	
sd16-1-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-8  9 }	
	
sd16-1-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-8  10 }	
	

sd16-1-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-8  11 }		

sd16-1-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-8  12 }	

sd16-1-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-8  13 }		

sd16-1-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-8  14 }	

	--
--	sd16-1
--    	

sd16-1-9Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-9  1 }

sd16-1-9Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-9  2 }

sd16-1-9Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-9  3 }

sd16-1-9Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-9  4 }
	
	
sd16-1-9FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-9  5 }		
	
	
sd16-1-9Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-9  6 }		
	
	
	
sd16-1-9EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-9  7 }		
	
sd16-1-9VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-9  8 }		
	
sd16-1-9VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-9  9 }	
	
sd16-1-9CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-9  10 }	
	

sd16-1-9CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-9  11 }		

sd16-1-9Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-9  12 }	

sd16-1-9ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-9  13 }		

sd16-1-9UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-9  14 }	

	
--
--	sd16-1
--    	

sd16-1-10Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-10  1 }

sd16-1-10Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-10  2 }

sd16-1-10Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-10  3 }

sd16-1-10Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-10  4 }
	
	
sd16-1-10FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-10  5 }		
	
	
sd16-1-10Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-10  6 }		
	
	
	
sd16-1-10EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-10  7 }		
	
sd16-1-10VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-10  8 }		
	
sd16-1-10VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-10  9 }	
	
sd16-1-10CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-10  10 }	
	

sd16-1-10CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-10  11 }		

sd16-1-10Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-10  12 }	

sd16-1-10ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-10  13 }		

sd16-1-10UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-10  14 }	

	
--
--	sd16-1
--    	

sd16-1-11Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-11  1 }

sd16-1-11Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-11  2 }

sd16-1-11Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-11  3 }

sd16-1-11Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-11  4 }
	
	
sd16-1-11FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-11  5 }		
	
	
sd16-1-11Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-11  6 }		
	
	
	
sd16-1-11EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-11  7 }		
	
sd16-1-11VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-11  8 }		
	
sd16-1-11VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-11  9 }	
	
sd16-1-11CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-11  10 }	
	

sd16-1-11CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-11  11 }		

sd16-1-11Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-11  12 }	

sd16-1-11ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-11  13 }		

sd16-1-11UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-11  14 }	

	
--
--	sd16-1
--    	

sd16-1-12Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-12  1 }

sd16-1-12Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-12  2 }

sd16-1-12Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-12  3 }

sd16-1-12Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-12  4 }
	
	
sd16-1-12FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-12  5 }		
	
	
sd16-1-12Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-12  6 }		
	
	
	
sd16-1-12EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-12  7 }		
	
sd16-1-12VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-12  8 }		
	
sd16-1-12VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-12  9 }	
	
sd16-1-12CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-12  10 }	
	

sd16-1-12CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-12  11 }		

sd16-1-12Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-12  12 }	

sd16-1-12ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-12  13 }		

sd16-1-12UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-12  14 }	

	
--
--	sd16-1
--    	

sd16-1-13Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-13  1 }

sd16-1-13Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-13  2 }

sd16-1-13Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-13  3 }

sd16-1-13Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-13  4 }
	
	
sd16-1-13FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-13  5 }		
	
	
sd16-1-13Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-13  6 }		
	
	
	
sd16-1-13EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-13  7 }		
	
sd16-1-13VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-13  8 }		
	
sd16-1-13VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-13  9 }	
	
sd16-1-13CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-13  10 }	
	

sd16-1-13CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-13  11 }		

sd16-1-13Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-13  12 }	

sd16-1-13ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-13  13 }		

sd16-1-13UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-13  14 }	

	
--
--	sd16-1
--    	

sd16-1-14Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-14  1 }

sd16-1-14Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-14  2 }

sd16-1-14Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-14  3 }

sd16-1-14Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-14  4 }
	
	
sd16-1-14FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-14  5 }		
	
	
sd16-1-14Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-14  6 }		
	
	
	
sd16-1-14EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-14  7 }		
	
sd16-1-14VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-14  8 }		
	
sd16-1-14VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-14  9 }	
	
sd16-1-14CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-14  10 }	
	

sd16-1-14CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-14  11 }		

sd16-1-14Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-14  12 }	

sd16-1-14ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-14  13 }		

sd16-1-14UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-14  14 }	

	
--
--	sd16-1
--    	

sd16-1-15Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-15  1 }

sd16-1-15Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-15  2 }

sd16-1-15Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-15  3 }

sd16-1-15Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-15  4 }
	
	
sd16-1-15FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-15  5 }		
	
	
sd16-1-15Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-15  6 }		
	
	
	
sd16-1-15EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-15  7 }		
	
sd16-1-15VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-15  8 }		
	
sd16-1-15VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-15  9 }	
	
sd16-1-15CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-15  10 }	
	

sd16-1-15CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-15  11 }		

sd16-1-15Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-15  12 }	

sd16-1-15ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-15  13 }		

sd16-1-15UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-15  14 }	

	
--
--	sd16-1
--    	

sd16-1-16Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-16  1 }

sd16-1-16Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-16  2 }

sd16-1-16Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-16  3 }

sd16-1-16Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-16  4 }
	
	
sd16-1-16FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-16  5 }		
	
	
sd16-1-16Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-16  6 }		
	
	
	
sd16-1-16EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-16  7 }		
	
sd16-1-16VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-16  8 }		
	
sd16-1-16VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-16  9 }	
	
sd16-1-16CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-16  10 }	
	

sd16-1-16CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-16  11 }		

sd16-1-16Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-16  12 }	

sd16-1-16ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-1-16  13 }		

sd16-1-16UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1-16  14 }	

	

sd16-1Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1  17 }	
    
sd16-1VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1  18 }

sd16-1VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1  19 }

sd16-1CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1  20 }

 sd16-1CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1  21 }
    
sd16-1Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1  22 }

sd16-1Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1  23 }

sd16-1TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1  24 }

sd16-1TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1  25 }

sd16-1Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1  26 }

sd16-1HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1  27 }

sd16-1HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1  28 }

sd16-1Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1  29 }

sd16-1Event2 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-1  30 }

--
--	sd16-2
--    



sd16-2-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-2  1 }

sd16-2-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-2  2 }

sd16-2-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-2  3 }

sd16-2-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-2  4 }
	
	
sd16-2-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-2  5 }		
	
	
sd16-2-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-2  6 }		

	
sd16-2-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-2  7 }		
	
sd16-2-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-2  8 }		
	
sd16-2-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-2  9 }	
	
sd16-2-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-2  10 }	
	

sd16-2-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-2  11 }		

	
sd16-2-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-2  12 }	

sd16-2-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-2-2  13 }	

sd16-2-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-2  14 }	

	
--
--	sd16-2
--    
	

sd16-2-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-3  1 }

sd16-2-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-3  2 }

sd16-2-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-3  3 }

sd16-2-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-3  4 }
	
	
sd16-2-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-3  5 }		
	
	
sd16-2-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-3  6 }
	
	
sd16-2-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-3  7 }		
	
sd16-2-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-3  8 }		
	
sd16-2-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-3  9 }	
	
sd16-2-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-3  10 }	
	

sd16-2-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-3  11 }	


sd16-2-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-3  12 }	

sd16-2-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-2-3  13 }	

sd16-2-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-3  14 }	

	
--
--	sd16-2
--    
	
	

sd16-2-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-4  1 }

sd16-2-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-4  2 }

sd16-2-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-4  3 }

sd16-2-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-4  4 }
	
	
sd16-2-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-4  5 }		
	
	
sd16-2-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-4  6 }		
	
	
sd16-2-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-4  7 }		
	
sd16-2-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-4  8 }		
	
sd16-2-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-4  9 }	
	
sd16-2-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-4  10 }	
	

sd16-2-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-4  11 }	

	
sd16-2-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-4  12 }	

sd16-2-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-2-4  13 }	

sd16-2-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-4  14 }	


	
--
--	sd16-2
--    

	
	

sd16-2-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-5  1 }

sd16-2-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-5  2 }

sd16-2-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-5  3 }

sd16-2-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-5  4 }
	
	
sd16-2-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-5  5 }		
	
	
sd16-2-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-5  6 }	
	
	
sd16-2-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-5  7 }		
	
sd16-2-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-5  8 }		
	
sd16-2-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-5  9 }	
	
sd16-2-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-5  10 }	
	

sd16-2-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-5  11 }	

sd16-2-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-5  12 }	

sd16-2-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-2-5  13 }		

sd16-2-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-5  14 }	

	
--
--	sd16-2
--    
	

sd16-2-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-6  1 }

sd16-2-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-6  2 }

sd16-2-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-6  3 }

sd16-2-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-6  4 }
	
	
sd16-2-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-6  5 }		
	
	
sd16-2-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-6  6 }	

	
sd16-2-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-6  7 }		
	
sd16-2-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-6  8 }		
	
sd16-2-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-6  9 }	
	
sd16-2-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-6  10 }	
	

sd16-2-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-6  11 }	

	
sd16-2-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-6  12 }	

sd16-2-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-2-6  13 }		

sd16-2-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-6  14 }	

	
--
--	sd16-2
--    

sd16-2-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-7  1 }

sd16-2-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-7  2 }

sd16-2-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-7  3 }

sd16-2-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-7  4 }
	
	
sd16-2-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-7  5 }		
	
	
sd16-2-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-7  6 }	


	
sd16-2-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-7  7 }		
	
sd16-2-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-7  8 }		
	
sd16-2-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-7  9 }	
	
sd16-2-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-7  10 }	
	

sd16-2-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-7  11 }		

sd16-2-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-7  12 }	

sd16-2-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-2-7  13 }	

sd16-2-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-7  14 }	
	
	
--
--	sd16-2
--    	

sd16-2-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-8  1 }

sd16-2-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-8  2 }

sd16-2-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-8  3 }

sd16-2-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-8  4 }
	
	
sd16-2-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-8  5 }		
	
	
sd16-2-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-8  6 }		
	
	
	
sd16-2-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-8  7 }		
	
sd16-2-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-8  8 }		
	
sd16-2-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-8  9 }	
	
sd16-2-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-8  10 }	
	

sd16-2-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-8  11 }		

sd16-2-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-8  12 }	

sd16-2-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-2-8  13 }		

sd16-2-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-8  14 }	

	--
--	sd16-2
--    	

sd16-2-9Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-9  1 }

sd16-2-9Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-9  2 }

sd16-2-9Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-9  3 }

sd16-2-9Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-9  4 }
	
	
sd16-2-9FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-9  5 }		
	
	
sd16-2-9Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-9  6 }		
	
	
	
sd16-2-9EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-9  7 }		
	
sd16-2-9VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-9  8 }		
	
sd16-2-9VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-9  9 }	
	
sd16-2-9CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-9  10 }	
	

sd16-2-9CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-9  11 }		

sd16-2-9Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-9  12 }	

sd16-2-9ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-2-9  13 }		

sd16-2-9UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-9  14 }	

	
--
--	sd16-2
--    	

sd16-2-10Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-10  1 }

sd16-2-10Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-10  2 }

sd16-2-10Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-10  3 }

sd16-2-10Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-10  4 }
	
	
sd16-2-10FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-10  5 }		
	
	
sd16-2-10Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-10  6 }		
	
	
	
sd16-2-10EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-10  7 }		
	
sd16-2-10VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-10  8 }		
	
sd16-2-10VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-10  9 }	
	
sd16-2-10CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-10  10 }	
	

sd16-2-10CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-10  11 }		

sd16-2-10Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-10  12 }	

sd16-2-10ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-2-10  13 }		

sd16-2-10UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-10  14 }	

	
--
--	sd16-2
--    	

sd16-2-11Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-11  1 }

sd16-2-11Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-11  2 }

sd16-2-11Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-11  3 }

sd16-2-11Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-11  4 }
	
	
sd16-2-11FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-11  5 }		
	
	
sd16-2-11Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-11  6 }		
	
	
	
sd16-2-11EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-11  7 }		
	
sd16-2-11VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-11  8 }		
	
sd16-2-11VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-11  9 }	
	
sd16-2-11CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-11  10 }	
	

sd16-2-11CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-11  11 }		

sd16-2-11Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-11  12 }	

sd16-2-11ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-2-11  13 }		

sd16-2-11UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-11  14 }	

	
--
--	sd16-2
--    	

sd16-2-12Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-12  1 }

sd16-2-12Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-12  2 }

sd16-2-12Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-12  3 }

sd16-2-12Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-12  4 }
	
	
sd16-2-12FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-12  5 }		
	
	
sd16-2-12Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-12  6 }		
	
	
	
sd16-2-12EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-12  7 }		
	
sd16-2-12VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-12  8 }		
	
sd16-2-12VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-12  9 }	
	
sd16-2-12CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-12  10 }	
	

sd16-2-12CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-12  11 }		

sd16-2-12Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-12  12 }	

sd16-2-12ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-2-12  13 }		

sd16-2-12UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-12  14 }	

	
--
--	sd16-2
--    	

sd16-2-13Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-13  1 }

sd16-2-13Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-13  2 }

sd16-2-13Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-13  3 }

sd16-2-13Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-13  4 }
	
	
sd16-2-13FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-13  5 }		
	
	
sd16-2-13Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-13  6 }		
	
	
	
sd16-2-13EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-13  7 }		
	
sd16-2-13VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-13  8 }		
	
sd16-2-13VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-13  9 }	
	
sd16-2-13CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-13  10 }	
	

sd16-2-13CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-13  11 }		

sd16-2-13Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-13  12 }	

sd16-2-13ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-2-13  13 }		

sd16-2-13UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-13  14 }	

	
--
--	sd16-2
--    	

sd16-2-14Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-14  1 }

sd16-2-14Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-14  2 }

sd16-2-14Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-14  3 }

sd16-2-14Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-14  4 }
	
	
sd16-2-14FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-14  5 }		
	
	
sd16-2-14Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-14  6 }		
	
	
	
sd16-2-14EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-14  7 }		
	
sd16-2-14VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-14  8 }		
	
sd16-2-14VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-14  9 }	
	
sd16-2-14CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-14  10 }	
	

sd16-2-14CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-14  11 }		

sd16-2-14Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-14  12 }	

sd16-2-14ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-2-14  13 }		

sd16-2-14UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-14  14 }	

	
--
--	sd16-2
--    	

sd16-2-15Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-15  1 }

sd16-2-15Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-15  2 }

sd16-2-15Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-15  3 }

sd16-2-15Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-15  4 }
	
	
sd16-2-15FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-15  5 }		
	
	
sd16-2-15Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-15  6 }		
	
	
	
sd16-2-15EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-15  7 }		
	
sd16-2-15VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-15  8 }		
	
sd16-2-15VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-15  9 }	
	
sd16-2-15CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-15  10 }	
	

sd16-2-15CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-15  11 }		

sd16-2-15Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-15  12 }	

sd16-2-15ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-2-15  13 }		

sd16-2-15UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-15  14 }	

	
--
--	sd16-2
--    	

sd16-2-16Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-16  1 }

sd16-2-16Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-16  2 }

sd16-2-16Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-16  3 }

sd16-2-16Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-16  4 }
	
	
sd16-2-16FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-16  5 }		
	
	
sd16-2-16Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-16  6 }		
	
	
	
sd16-2-16EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-16  7 }		
	
sd16-2-16VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-16  8 }		
	
sd16-2-16VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-16  9 }	
	
sd16-2-16CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-16  10 }	
	

sd16-2-16CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-16  11 }		

sd16-2-16Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-16  12 }	

sd16-2-16ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-2-16  13 }		

sd16-2-16UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2-16  14 }	

	

sd16-2Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2  17 }	
    
sd16-2VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2  18 }

sd16-2VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2  19 }

sd16-2CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2  20 }

 sd16-2CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2  21 }
    
sd16-2Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2  22 }

sd16-2Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2  23 }

sd16-2TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2  24 }

sd16-2TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2  25 }

sd16-2Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2  26 }

sd16-2HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2  27 }

sd16-2HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2  28 }

sd16-2Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2  29 }

sd16-2Event2 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-2  30 }

--
--	sd16-3
--    



sd16-3-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-2  1 }

sd16-3-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-2  2 }

sd16-3-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-2  3 }

sd16-3-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-2  4 }
	
	
sd16-3-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-2  5 }		
	
	
sd16-3-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-2  6 }		

	
sd16-3-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-2  7 }		
	
sd16-3-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-2  8 }		
	
sd16-3-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-2  9 }	
	
sd16-3-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-2  10 }	
	

sd16-3-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-2  11 }		

	
sd16-3-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-2  12 }	

sd16-3-2ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-3-2  13 }	

sd16-3-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-2  14 }	

	
--
--	sd16-3
--    
	

sd16-3-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-3  1 }

sd16-3-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-3  2 }

sd16-3-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-3  3 }

sd16-3-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-3  4 }
	
	
sd16-3-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-3  5 }		
	
	
sd16-3-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-3  6 }
	
	
sd16-3-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-3  7 }		
	
sd16-3-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-3  8 }		
	
sd16-3-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-3  9 }	
	
sd16-3-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-3  10 }	
	

sd16-3-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-3  11 }	


sd16-3-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-3  12 }	

sd16-3-3ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-3-3  13 }	

sd16-3-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-3  14 }	

	
--
--	sd16-3
--    
	
	

sd16-3-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-4  1 }

sd16-3-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-4  2 }

sd16-3-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-4  3 }

sd16-3-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-4  4 }
	
	
sd16-3-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-4  5 }		
	
	
sd16-3-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-4  6 }		
	
	
sd16-3-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-4  7 }		
	
sd16-3-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-4  8 }		
	
sd16-3-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-4  9 }	
	
sd16-3-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-4  10 }	
	

sd16-3-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-4  11 }	

	
sd16-3-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-4  12 }	

sd16-3-4ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-3-4  13 }	

sd16-3-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-4  14 }	


	
--
--	sd16-3
--    

	
	

sd16-3-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-5  1 }

sd16-3-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-5  2 }

sd16-3-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-5  3 }

sd16-3-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-5  4 }
	
	
sd16-3-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-5  5 }		
	
	
sd16-3-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-5  6 }	
	
	
sd16-3-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-5  7 }		
	
sd16-3-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-5  8 }		
	
sd16-3-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-5  9 }	
	
sd16-3-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-5  10 }	
	

sd16-3-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-5  11 }	

sd16-3-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-5  12 }	

sd16-3-5ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-3-5  13 }		

sd16-3-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-5  14 }	

	
--
--	sd16-3
--    
	

sd16-3-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-6  1 }

sd16-3-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-6  2 }

sd16-3-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-6  3 }

sd16-3-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-6  4 }
	
	
sd16-3-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-6  5 }		
	
	
sd16-3-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-6  6 }	

	
sd16-3-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-6  7 }		
	
sd16-3-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-6  8 }		
	
sd16-3-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-6  9 }	
	
sd16-3-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-6  10 }	
	

sd16-3-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-6  11 }	

	
sd16-3-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-6  12 }	

sd16-3-6ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-3-6  13 }		

sd16-3-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-6  14 }	

	
--
--	sd16-3
--    

sd16-3-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-7  1 }

sd16-3-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-7  2 }

sd16-3-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-7  3 }

sd16-3-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-7  4 }
	
	
sd16-3-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-7  5 }		
	
	
sd16-3-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-7  6 }	


	
sd16-3-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-7  7 }		
	
sd16-3-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-7  8 }		
	
sd16-3-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-7  9 }	
	
sd16-3-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-7  10 }	
	

sd16-3-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-7  11 }		

sd16-3-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-7  12 }	

sd16-3-7ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-3-7  13 }	

sd16-3-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-7  14 }	
	
	
--
--	sd16-3
--    	

sd16-3-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-8  1 }

sd16-3-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-8  2 }

sd16-3-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-8  3 }

sd16-3-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-8  4 }
	
	
sd16-3-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-8  5 }		
	
	
sd16-3-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-8  6 }		
	
	
	
sd16-3-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-8  7 }		
	
sd16-3-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-8  8 }		
	
sd16-3-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-8  9 }	
	
sd16-3-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-8  10 }	
	

sd16-3-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-8  11 }		

sd16-3-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-8  12 }	

sd16-3-8ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-3-8  13 }		

sd16-3-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-8  14 }	

	--
--	sd16-3
--    	

sd16-3-9Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-9  1 }

sd16-3-9Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-9  2 }

sd16-3-9Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-9  3 }

sd16-3-9Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-9  4 }
	
	
sd16-3-9FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-9  5 }		
	
	
sd16-3-9Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-9  6 }		
	
	
	
sd16-3-9EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-9  7 }		
	
sd16-3-9VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-9  8 }		
	
sd16-3-9VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-9  9 }	
	
sd16-3-9CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-9  10 }	
	

sd16-3-9CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-9  11 }		

sd16-3-9Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-9  12 }	

sd16-3-9ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-3-9  13 }		

sd16-3-9UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-9  14 }	

	
--
--	sd16-3
--    	

sd16-3-10Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-10  1 }

sd16-3-10Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-10  2 }

sd16-3-10Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-10  3 }

sd16-3-10Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-10  4 }
	
	
sd16-3-10FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-10  5 }		
	
	
sd16-3-10Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-10  6 }		
	
	
	
sd16-3-10EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-10  7 }		
	
sd16-3-10VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-10  8 }		
	
sd16-3-10VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-10  9 }	
	
sd16-3-10CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-10  10 }	
	

sd16-3-10CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-10  11 }		

sd16-3-10Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-10  12 }	

sd16-3-10ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-3-10  13 }		

sd16-3-10UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-10  14 }	

	
--
--	sd16-3
--    	

sd16-3-11Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-11  1 }

sd16-3-11Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-11  2 }

sd16-3-11Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-11  3 }

sd16-3-11Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-11  4 }
	
	
sd16-3-11FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-11  5 }		
	
	
sd16-3-11Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-11  6 }		
	
	
	
sd16-3-11EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-11  7 }		
	
sd16-3-11VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-11  8 }		
	
sd16-3-11VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-11  9 }	
	
sd16-3-11CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-11  10 }	
	

sd16-3-11CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-11  11 }		

sd16-3-11Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-11  12 }	

sd16-3-11ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-3-11  13 }		

sd16-3-11UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-11  14 }	

	
--
--	sd16-3
--    	

sd16-3-12Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-12  1 }

sd16-3-12Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-12  2 }

sd16-3-12Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-12  3 }

sd16-3-12Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-12  4 }
	
	
sd16-3-12FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-12  5 }		
	
	
sd16-3-12Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-12  6 }		
	
	
	
sd16-3-12EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-12  7 }		
	
sd16-3-12VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-12  8 }		
	
sd16-3-12VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-12  9 }	
	
sd16-3-12CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-12  10 }	
	

sd16-3-12CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-12  11 }		

sd16-3-12Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-12  12 }	

sd16-3-12ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-3-12  13 }		

sd16-3-12UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-12  14 }	

	
--
--	sd16-3
--    	

sd16-3-13Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-13  1 }

sd16-3-13Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-13  2 }

sd16-3-13Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-13  3 }

sd16-3-13Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-13  4 }
	
	
sd16-3-13FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-13  5 }		
	
	
sd16-3-13Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-13  6 }		
	
	
	
sd16-3-13EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-13  7 }		
	
sd16-3-13VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-13  8 }		
	
sd16-3-13VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-13  9 }	
	
sd16-3-13CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-13  10 }	
	

sd16-3-13CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-13  11 }		

sd16-3-13Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-13  12 }	

sd16-3-13ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-3-13  13 }		

sd16-3-13UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-13  14 }	

	
--
--	sd16-3
--    	

sd16-3-14Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-14  1 }

sd16-3-14Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-14  2 }

sd16-3-14Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-14  3 }

sd16-3-14Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-14  4 }
	
	
sd16-3-14FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-14  5 }		
	
	
sd16-3-14Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-14  6 }		
	
	
	
sd16-3-14EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-14  7 }		
	
sd16-3-14VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-14  8 }		
	
sd16-3-14VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-14  9 }	
	
sd16-3-14CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-14  10 }	
	

sd16-3-14CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-14  11 }		

sd16-3-14Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-14  12 }	

sd16-3-14ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-3-14  13 }		

sd16-3-14UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-14  14 }	

	
--
--	sd16-3
--    	

sd16-3-15Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-15  1 }

sd16-3-15Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-15  2 }

sd16-3-15Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-15  3 }

sd16-3-15Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-15  4 }
	
	
sd16-3-15FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-15  5 }		
	
	
sd16-3-15Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-15  6 }		
	
	
	
sd16-3-15EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-15  7 }		
	
sd16-3-15VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-15  8 }		
	
sd16-3-15VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-15  9 }	
	
sd16-3-15CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-15  10 }	
	

sd16-3-15CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-15  11 }		

sd16-3-15Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-15  12 }	

sd16-3-15ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-3-15  13 }		

sd16-3-15UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-15  14 }	

	
--
--	sd16-3
--    	

sd16-3-16Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-16  1 }

sd16-3-16Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-16  2 }

sd16-3-16Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-16  3 }

sd16-3-16Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-16  4 }
	
	
sd16-3-16FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-16  5 }		
	
	
sd16-3-16Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-16  6 }		
	
	
	
sd16-3-16EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-16  7 }		
	
sd16-3-16VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-16  8 }		
	
sd16-3-16VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-16  9 }	
	
sd16-3-16CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-16  10 }	
	

sd16-3-16CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-16  11 }		

sd16-3-16Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-16  12 }	

sd16-3-16ResetStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enter 'Active' to reset sd16 channel output."
    DEFVAL { "" }
    ::= { sd16-3-16  13 }		

sd16-3-16UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3-16  14 }	

	

sd16-3Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3  17 }	
    
sd16-3VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3  18 }

sd16-3VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3  19 }

sd16-3CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3  20 }

 sd16-3CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3  21 }
    
sd16-3Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3  22 }

sd16-3Temperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3  23 }

sd16-3TemperatureLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3  24 }

sd16-3TemperatureUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3  25 }

sd16-3Humidity OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3  26 }

sd16-3HumidityLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3  27 }

sd16-3HumidityUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3  28 }

sd16-3Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3  29 }

sd16-3Event2 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { sd16-3  30 }


END
