LSPNL4MIB DEFINITIONS ::= BEGIN

--
-- Top-level infrastructure of the Net-SNMP project enterprise MIB tree
--

IMPORTS
    MODULE-IDENTITY, enterprises          	FROM SNMPv2-SMI
    MODULE-IDENTITY, OBJECT-TYPE, Integer32,
    NOTIFICATION-TYPE                       FROM SNMPv2-SMI
    SnmpAdminString                         FROM SNMP-FRAMEWORK-MIB
    netSnmp                                 FROM NET-SNMP-MIB
    RowStatus, StorageType, DisplayString   FROM SNMPv2-TC
    InetAddressType, InetAddress            FROM INET-ADDRESS-MIB
;
LSPNL4MIB MODULE-IDENTITY
    LAST-UPDATED "201404181010Z"
    ORGANIZATION "LifeSafety Power, Inc. "
    CONTACT-INFO    
     "http://www.lifesafetypower.com/
	 
	  EMail: gliu@lifesafetypower.com
	 "
    DESCRIPTION
    "This is the MIB Module for NL4 and NL2 objects for managing NL4/NL2 device."

	REVISION	"201408291010Z"
	DESCRIPTION
	"Updated to support Net-SNMP compile."
    ::= { enterprises 42520}
    


NL4MIB OBJECT IDENTIFIER ::= {LSPNL4MIB 3}  




fp1         	OBJECT IDENTIFIER ::= { NL4MIB 1}
fp2        		OBJECT IDENTIFIER ::= { NL4MIB 2}
nac1        	OBJECT IDENTIFIER ::= { NL4MIB 4}
nac2         	OBJECT IDENTIFIER ::= { NL4MIB 5}
m8-1          	OBJECT IDENTIFIER ::= { NL4MIB 7}
m8-1-1  		OBJECT IDENTIFIER ::= { m8-1  1}
m8-1-2  		OBJECT IDENTIFIER ::= { m8-1  2}
m8-1-3  		OBJECT IDENTIFIER ::= { m8-1  3}
m8-1-4  		OBJECT IDENTIFIER ::= { m8-1  4}
m8-1-5  		OBJECT IDENTIFIER ::= { m8-1  5}
m8-1-6  		OBJECT IDENTIFIER ::= { m8-1  6}
m8-1-7  		OBJECT IDENTIFIER ::= { m8-1  7}
m8-1-8  		OBJECT IDENTIFIER ::= { m8-1  8}
m8-2          	OBJECT IDENTIFIER ::= { NL4MIB 8}
m8-2-1  		OBJECT IDENTIFIER ::= { m8-2  1}
m8-2-2  		OBJECT IDENTIFIER ::= { m8-2  2}
m8-2-3  		OBJECT IDENTIFIER ::= { m8-2  3}
m8-2-4  		OBJECT IDENTIFIER ::= { m8-2  4}
m8-2-5  		OBJECT IDENTIFIER ::= { m8-2  5}
m8-2-6  		OBJECT IDENTIFIER ::= { m8-2  6}
m8-2-7  		OBJECT IDENTIFIER ::= { m8-2  7}
m8-2-8  		OBJECT IDENTIFIER ::= { m8-2  8}
m8-3          	OBJECT IDENTIFIER ::= { NL4MIB 9}
m8-3-1  		OBJECT IDENTIFIER ::= { m8-3  1}
m8-3-2  		OBJECT IDENTIFIER ::= { m8-3  2}
m8-3-3  		OBJECT IDENTIFIER ::= { m8-3  3}
m8-3-4  		OBJECT IDENTIFIER ::= { m8-3  4}
m8-3-5  		OBJECT IDENTIFIER ::= { m8-3  5}
m8-3-6  		OBJECT IDENTIFIER ::= { m8-3  6}
m8-3-7  		OBJECT IDENTIFIER ::= { m8-3  7}
m8-3-8  		OBJECT IDENTIFIER ::= { m8-3  8}
netlink       	OBJECT IDENTIFIER ::= { NL4MIB 10}

NL4Traps       	OBJECT IDENTIFIER ::= { LSPNL4MIB 4}




--
--	FP1
--    
FP1Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Time."
    DEFVAL { "" }
    ::= { fp1  1 }

FP1DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FPO ID."
    DEFVAL { "" }
    ::= { fp1  2 }

FP1ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply Model, Such as FPO75-25, FPO150-100, FPO250-200."
    DEFVAL { "" }
    ::= { fp1  3 }

FP1SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply system fault status."
    DEFVAL { "" }
    ::= { fp1  4 }

FP1ACFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply AC lost status, No or Yes."
    DEFVAL { "" }
    ::= { fp1  5 }

FP1FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI status."
    DEFVAL { "" }
    ::= { fp1  6 }

FP1OutputLatchingOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI latch status."
    DEFVAL { "" }
    ::= { fp1  7 }
    
FP1ACInputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC input voltage."
    DEFVAL { "" }
    ::= { fp1  8 }

FP1OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output voltage."
    DEFVAL { "" }
    ::= { fp1  9 }
    
FP1OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output Current."
    DEFVAL { "" }
    ::= { fp1  10 }
    

FP1BatteryVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System battery voltage."
    DEFVAL { "" }
    ::= { fp1  11 }

FP1BatteryChargeCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery charge current."
    DEFVAL { "" }
    ::= { fp1  12 }
    
FP1BatteryFaultDetect OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Fault Detect."
    DEFVAL { "" }
    ::= { fp1  13 }

FP1TotalPowerupTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power supply total runtime."
    DEFVAL { "" }
    ::= { fp1  14 }

FP1BatteryInstalledTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery install hours."
    DEFVAL { "" }
    ::= { fp1  15 }

FP1NumberOfACFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC lost count."
    DEFVAL { "" }
    ::= { fp1  16 }

FP1NumberOfSystemFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System fault count."
    DEFVAL { "" }
    ::= { fp1  17 }
	
	
FP1RatedBatteryLife OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "FPO battery lifetime."
    DEFVAL { "" }
    ::= { fp1  18 }	

	
FP1RatedCapacity  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery capacity."
    DEFVAL { "" }
    ::= { fp1  19 }	
	
		
FP1BatteryStateOfCharge OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "The FPO battery state of charge."
    DEFVAL { "" }
    ::= { fp1  20 }	


FP1BatteryStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable calculate battery state of charge. Set Value: Enabled or Disabled"
    DEFVAL { "" }
    ::= { fp1  21 }		
		
FP1BatteryTestStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery discharge test status, Active or Inactive. Set Value: Testing or Inactive"
    DEFVAL { "" }
    ::= { fp1  22 }

FP1BatteryLastTestDate OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test date."
    DEFVAL { "" }
    ::= { fp1  23 }

FP1BatteryLastTestDischargeTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test time."
    DEFVAL { "" }
    ::= { fp1  24 }
    
FP1RepeatTestInterval OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Repeat Test Interval."
    DEFVAL { "" }
    ::= { fp1  25 }
    
FP1Version	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FP1 Ver."
    DEFVAL { "" }
    ::= { fp1  26 }  
    
FP1SystemFaultDescription	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Fault Description."
    DEFVAL { "" }
    ::= { fp1  27 }         
    
 FP1BatteryTestsPerformed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Performed."
    DEFVAL { "" }
    ::= { fp1  28 }   

FP1BatteryTestsFailed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Failed."
    DEFVAL { "" }
    ::= { fp1  29 }  

   FP1RequiredBatteryRuntime	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS   read-write
    STATUS      current
    DESCRIPTION
    "Required Battery Runtime."
    DEFVAL { "" }
    ::= { fp1  30 }  

    FP1ActualStandby	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Actual Standby."
    DEFVAL { "" }
    ::= { fp1  31 }  

--
--	FP2
--    
FP2Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { fp2  1 }

FP2DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { fp2  2 }

FP2ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { fp2  3 }
FP2SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply system fault status."
    DEFVAL { "" }
    ::= { fp2  4 }

FP2ACFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply AC lost status, No or Yes."
    DEFVAL { "" }
    ::= { fp2  5 }

FP2FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI status."
    DEFVAL { "" }
    ::= { fp2  6 }

FP2OutputLatchingOnFAI OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI latch status."
    DEFVAL { "" }
    ::= { fp2  7 }
    
FP2ACInputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC input voltage."
    DEFVAL { "" }
    ::= { fp2  8 }

FP2OutputVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output voltage."
    DEFVAL { "" }
    ::= { fp2  9 }
    
FP2OutputCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power Supply output Current."
    DEFVAL { "" }
    ::= { fp2  10 }
    

FP2BatteryVoltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System battery voltage."
    DEFVAL { "" }
    ::= { fp2  11 }

FP2BatteryChargeCurrent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery charge current."
    DEFVAL { "" }
    ::= { fp2  12 }
    
FP2BatteryFaultDetect OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Fault Detect."
    DEFVAL { "" }
    ::= { fp2  13 }

FP2TotalPowerupTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Power supply total runtime."
    DEFVAL { "" }
    ::= { fp2  14 }

FP2BatteryInstalledTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery install hours."
    DEFVAL { "" }
    ::= { fp2  15 }

FP2NumberOfACFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "AC lost count."
    DEFVAL { "" }
    ::= { fp2  16 }

FP2NumberOfSystemFaultsDetected OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System fault count."
    DEFVAL { "" }
    ::= { fp2  17 }
	
	
FP2RatedBatteryLife OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "FPO battery lifetime."
    DEFVAL { "" }
    ::= { fp2  18 }	

	
FP2RatedCapacity  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery capacity."
    DEFVAL { "" }
    ::= { fp2  19 }	
	
		
FP2BatteryStateOfCharge OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "The FPO battery state of charge."
    DEFVAL { "" }
    ::= { fp2  20 }	


FP2BatteryStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable calculate battery state of charge."
    DEFVAL { "" }
    ::= { fp2  21 }		
		
FP2BatteryTestStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Battery discharge test status, Active or Inactive"
    DEFVAL { "" }
    ::= { fp2  22 }

FP2BatteryLastTestDate OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test date."
    DEFVAL { "" }
    ::= { fp2  23 }

FP2BatteryLastTestDischargeTime OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery last discharge test time."
    DEFVAL { "" }
    ::= { fp2  24 }
    
FP2RepeatTestInterval OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Repeat Test Interval."
    DEFVAL { "" }
    ::= { fp2  25 }
    
 FP2Version	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "FP2 Ver."
    DEFVAL { "" }
    ::= { fp2  26 }  
    
FP2SystemFaultDescription	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Fault Description."
    DEFVAL { "" }
    ::= { fp2  27 }    
   
     FP2BatteryTestsPerformed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Performed."
    DEFVAL { "" }
    ::= { fp2  28 }   

FP2BatteryTestsFailed	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Battery Tests Failed."
    DEFVAL { "" }
    ::= { fp2  29 }  

   FP2RequiredBatteryRuntime	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Required Battery Runtime."
    DEFVAL { "" }
    ::= { fp2  30 }  

    FP2ActualStandby	OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Actual Standby."
    DEFVAL { "" }
    ::= { fp2  31 } 

--
--	NAC1
--    
NAC1Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Time."
    DEFVAL { "" }
    ::= { nac1  1 }

NAC1DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "NAC device ID."
    DEFVAL { "" }
    ::= { nac1  2 }

NAC1ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Device model is N24,NULL for none device detected."
    DEFVAL { "" }
    ::= { nac1  3 }

NAC1SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Fault Status, No or Yes."
    DEFVAL { "" }
    ::= { nac1  4 }

NAC1FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI Status, Active or Inactive"
    DEFVAL { "" }
    ::= { nac1  5 }

NAC1ModeStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "NAC model, Supervisory or Alarm model."
    DEFVAL { "" }
    ::= { nac1  6 }
    
NAC1Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "NAC Ver."
    DEFVAL { "" }
    ::= { nac1  7 }    

--
--	NAC2
--    
NAC2Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nac2  1 }

NAC2DeviceID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nac2  2 }

NAC2ModNumber OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nac2  3 }

NAC2SystemFaultStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nac2  4 }

NAC2FAIStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nac2  5 }

NAC2ModeStatus OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nac2  6 }
    
NAC2Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { nac2  7 }    

		
--
--	m8-1
--    		

m8-1-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- description, it is entered by user from GUI"
    DEFVAL { "" }
    ::= { m8-1-1  1 }

m8-1-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output voltage."
    DEFVAL { "" }
    ::= { m8-1-1  2 }

m8-1-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output current."
    DEFVAL { "" }
    ::= { m8-1-1  3 }

m8-1-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- output power"
    DEFVAL { "" }
    ::= { m8-1-1  4 }
	
m8-1-1PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- power supply."
    DEFVAL { "" }
    ::= { m8-1-1  5 }	
	
	
m8-1-1ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- Output response to control input, Active, Inactive or Disable."
    DEFVAL { "" }
    ::= { m8-1-1  6 }		
	
m8-1-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System FAI state, Active or Inactive."
    DEFVAL { "" }
    ::= { m8-1-1  7 }		
	
	
m8-1-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "- status, Normal, Fault or no use."
    DEFVAL { "" }
    ::= { m8-1-1  8 }

m8-1-1CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- control Input Type, Normally Open, Normally Closed,
    Open Collector, Voltage, Disabled."
    DEFVAL { "" }
    ::= { m8-1-1  9 }	
	
	
m8-1-1OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- output load type, Maglock, Fail-safe Strike, 
    Fail-secure Strike, Constant ON."
    DEFVAL { "" }
    ::= { m8-1-1  10 }	
	
m8-1-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on FAI Activation, Yes or No."
    DEFVAL { "" }
    ::= { m8-1-1  11 }	
	
	
m8-1-1UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- unlock on AC loss, Yes or No."
    DEFVAL { "" }
    ::= { m8-1-1  12 }	
	
m8-1-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Email alert on Fault, Yes or No."
    DEFVAL { "" }
    ::= { m8-1-1  13 }		
	
m8-1-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage lower limit."
    DEFVAL { "" }
    ::= { m8-1-1  14 }		
	
m8-1-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- voltage upper limit."
    DEFVAL { "" }
    ::= { m8-1-1  15 }	
	
m8-1-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current lower limit."
    DEFVAL { "" }
    ::= { m8-1-1  16 }	
	

m8-1-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- current upper limit."
    DEFVAL { "" }
    ::= { m8-1-1  17 }	

m8-1-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "Enable or Disable M8 -."
    DEFVAL { "" }
    ::= { m8-1-1  18 }		
	
	
--
--	m8-1
--    



m8-1-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  1 }

m8-1-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  2 }

m8-1-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  3 }

m8-1-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  4 }
	
m8-1-2PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  5 }	
	
	
m8-1-2ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  6 }		
	
m8-1-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  7 }		
	
	
m8-1-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  8 }		

m8-1-2CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  9 }	
	
m8-1-2OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  10 }	

m8-1-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  11 }	
	
	
m8-1-2UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  12 }	
	
m8-1-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  13 }		
	
m8-1-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  14 }		
	
m8-1-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  15 }	
	
m8-1-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  16 }	
	

m8-1-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  17 }		

	
m8-1-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-2  18 }	
	
--
--	m8-1
--    
	

m8-1-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  1 }

m8-1-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  2 }

m8-1-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  3 }

m8-1-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  4 }
	
m8-1-3PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  5 }	
	
	
m8-1-3ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  6 }		
	
m8-1-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  7 }		
	
	
m8-1-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  8 }
	

m8-1-3CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  9 }


m8-1-3OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  10 }	
	

m8-1-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  11 }	
	
	
m8-1-3UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  12 }	
	
m8-1-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  13 }		
	
m8-1-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  14 }		
	
m8-1-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  15 }	
	
m8-1-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  16 }	
	

m8-1-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  17 }	


m8-1-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-3  18 }	
	
--
--	m8-1
--    
	
	

m8-1-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  1 }

m8-1-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  2 }

m8-1-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  3 }

m8-1-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  4 }
	
m8-1-4PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  5 }	
	
	
m8-1-4ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  6 }		
	
m8-1-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  7 }		
	
	
m8-1-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  8 }		
	

m8-1-4CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  9 }	
	

m8-1-4OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  10 }	


m8-1-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  11 }	
	
	
m8-1-4UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  12 }	
	
m8-1-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  13 }		
	
m8-1-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  14 }		
	
m8-1-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  15 }	
	
m8-1-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  16 }	
	

m8-1-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  17 }	

	
m8-1-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-4  18 }	

	
--
--	m8-1
--    

	
	

m8-1-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  1 }

m8-1-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  2 }

m8-1-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  3 }

m8-1-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  4 }
	
m8-1-5PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  5 }	
	
	
m8-1-5ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  6 }		
	
m8-1-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  7 }		
	
	
m8-1-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  8 }	
	

m8-1-5CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  9 }
	
	
m8-1-5OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  10 }	
	
	
m8-1-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  11 }	
	
	
m8-1-5UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  12 }	
	
m8-1-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  13 }		
	
m8-1-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  14 }		
	
m8-1-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  15 }	
	
m8-1-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  16 }	
	

m8-1-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  17 }	

m8-1-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-5  18 }		
	
--
--	m8-1
--    
	

m8-1-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  1 }

m8-1-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  2 }

m8-1-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  3 }

m8-1-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  4 }
	
m8-1-6PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  5 }	
	
	
m8-1-6ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  6 }		
	
m8-1-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  7 }		
	
	
m8-1-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  8 }	


m8-1-6CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  9 }

	
m8-1-6OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  10 }	
	
m8-1-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  11 }	
	
	
m8-1-6UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  12 }	
	
m8-1-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  13 }		
	
m8-1-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  14 }		
	
m8-1-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  15 }	
	
m8-1-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  16 }	
	

m8-1-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  17 }	

	
m8-1-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-6  18 }		
	
--
--	m8-1
--    

m8-1-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  1 }

m8-1-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  2 }

m8-1-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  3 }

m8-1-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  4 }
	
m8-1-7PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  5 }	
	
	
m8-1-7ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  6 }		
	
m8-1-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  7 }		
	
	
m8-1-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  8 }	


m8-1-7CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  9 }

m8-1-7OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  10 }	

m8-1-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  11 }	
	
	
m8-1-7UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  12 }	
	
m8-1-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  13 }		
	
m8-1-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  14 }		
	
m8-1-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  15 }	
	
m8-1-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  16 }	
	

m8-1-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  17 }		

m8-1-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-7  18 }		
	
--
--	m8-1
--    	

m8-1-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  1 }

m8-1-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  2 }

m8-1-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  3 }

m8-1-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  4 }
	
m8-1-8PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  5 }	
	
	
m8-1-8ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  6 }		
	
m8-1-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  7 }		
	
	
m8-1-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  8 }		
	
	
m8-1-8CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  9 }


m8-1-8OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  10 }	

m8-1-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  11 }	
	
	
m8-1-8UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  12 }	
	
m8-1-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  13 }		
	
m8-1-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  14 }		
	
m8-1-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  15 }	
	
m8-1-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  16 }	
	

m8-1-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  17 }		

m8-1-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1-8  18 }		
	
m8-1Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-1  9 }	
    
m8-1VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Output Voltage Lower Limit Percent"
    DEFVAL { "" }
    ::= { m8-1  10 }

m8-1VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Output Voltage Upper Limit Percent"
    DEFVAL { "" }
    ::= { m8-1  11 }

m8-1CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Output Current Lower Limit Percent"
    DEFVAL { "" }
    ::= { m8-1  12 }

 m8-1CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Output Current Upper Limit Percent"
    DEFVAL { "" }
    ::= { m8-1  13 }
    
m8-1Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "- Output Limit Setting process, Active or Inactive."
    DEFVAL { "" }
    ::= { m8-1  14 }

--
--	M8-2
--    


m8-2-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  1 }

m8-2-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  2 }

m8-2-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  3 }

m8-2-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  4 }
	
m8-2-1PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  5 }	
	
	
m8-2-1ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  6 }		
	
m8-2-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  7 }		
	
	
m8-2-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  8 }		
	
	
m8-2-1CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  9 }	
	

m8-2-1OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  10 }	

m8-2-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  11 }	
	
	
m8-2-1UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  12 }	
	
m8-2-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  13 }		
	
m8-2-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  14 }		
	
m8-2-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  15 }	
	
m8-2-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  16 }	
	

m8-2-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  17 }		
	

m8-2-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-1  18 }		
	
	
--
--	M8-2
--    

m8-2-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  1 }

m8-2-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  2 }

m8-2-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  3 }

m8-2-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  4 }
	
m8-2-2PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  5 }	
	
	
m8-2-2ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  6 }		
	
m8-2-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  7 }		
	
	
m8-2-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  8 }		


m8-2-2CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  9 }		
	
m8-2-2OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  10 }	

m8-2-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  11 }	
	
	
m8-2-2UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  12 }	
	
m8-2-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  13 }		
	
m8-2-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  14 }		
	
m8-2-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  15 }	
	
m8-2-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  16 }	
	

m8-2-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  17 }		

m8-2-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-2  18 }		
	
--
--	M8-2
--    


m8-2-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  1 }

m8-2-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  2 }

m8-2-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  3 }

m8-2-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  4 }
	
m8-2-3PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  5 }	
	
	
m8-2-3ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  6 }		
	
m8-2-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  7 }		
	
	
m8-2-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  8 }		


m8-2-3CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  9 }	
	

m8-2-3OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  10 }	

m8-2-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  11 }	
	
	
m8-2-3UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  12 }	
	
m8-2-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  13 }		
	
m8-2-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  14 }		
	
m8-2-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  15 }	
	
m8-2-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  16 }	
	

m8-2-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  17 }	

	
m8-2-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-3  18 }		
	
--
--	M8-2
--    

	

m8-2-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  1 }

m8-2-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  2 }

m8-2-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  3 }

m8-2-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  4 }
	
m8-2-4PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  5 }	
	
	
m8-2-4ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  6 }		
	
m8-2-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  7 }		
	
	
m8-2-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  8 }		

	
m8-2-4CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  9 }


m8-2-4OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  10 }	

m8-2-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  11 }	
	
	
m8-2-4UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  12 }	
	
m8-2-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  13 }		
	
m8-2-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  14 }		
	
m8-2-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  15 }	
	
m8-2-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  16 }	
	

m8-2-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  17 }		


m8-2-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-4  18 }		
	
--
--	M8-2
--    	

m8-2-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  1 }

m8-2-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  2 }

m8-2-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  3 }

m8-2-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  4 }
	
m8-2-5PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  5 }	
	
	
m8-2-5ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  6 }		
	
m8-2-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  7 }		
	
	
m8-2-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  8 }	
	

m8-2-5CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  9 }
	
	
m8-2-5OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  10 }	

m8-2-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  11 }	
	
	
m8-2-5UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  12 }	
	
m8-2-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  13 }		
	
m8-2-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  14 }		
	
m8-2-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  15 }	
	
m8-2-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  16 }	
	

m8-2-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  17 }	

m8-2-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-5  18 }			
	
--
--	M8-2
--    

m8-2-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  1 }

m8-2-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  2 }

m8-2-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  3 }

m8-2-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  4 }
	
m8-2-6PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  5 }	
	
	
m8-2-6ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  6 }		
	
m8-2-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  7 }		
	
	
m8-2-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  8 }	


m8-2-6CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  9 }

	
m8-2-6OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  10 }	

m8-2-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  11 }	
	
	
m8-2-6UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  12 }	
	
m8-2-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  13 }		
	
m8-2-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  14 }		
	
m8-2-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  15 }	
	
m8-2-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  16 }	
	

m8-2-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  17 }	

m8-2-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-6  18 }			
	
--
--	M8-2
--    


m8-2-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  1 }

m8-2-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  2 }

m8-2-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  3 }

m8-2-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  4 }
	
m8-2-7PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  5 }	
	
	
m8-2-7ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  6 }		
	
m8-2-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  7 }		
	
	
m8-2-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  8 }	


m8-2-7CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  9 }

	
m8-2-7OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  10 }	

m8-2-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  11 }	
	
	
m8-2-7UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  12 }	
	
m8-2-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  13 }		
	
m8-2-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  14 }		
	
m8-2-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  15 }	
	
m8-2-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  16 }	
	

m8-2-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  17 }	

m8-2-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-7  18 }			
	
--
--	M8-2
--    	

m8-2-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  1 }

m8-2-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  2 }

m8-2-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  3 }

m8-2-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  4 }
	
m8-2-8PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  5 }	
	
	
m8-2-8ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  6 }		
	
m8-2-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  7 }		
	
	
m8-2-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  8 }		
	
	
m8-2-8CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  9 }


m8-2-8OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  10 }	

m8-2-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  11 }	
	
	
m8-2-8UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  12 }	
	
m8-2-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  13 }		
	
m8-2-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  14 }		
	
m8-2-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  15 }	
	
m8-2-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  16 }	
	

m8-2-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  17 }	

m8-2-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2-8  18 }			
	
m8-2Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2  9 }
    
m8-2VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2  10 }

m8-2VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2  11 }

m8-2CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2  12 }

 m8-2CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2  13 }
    
    
m8-2Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-2  14 }    
    


--
--	M8-3
--    


m8-3-1Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  1 }

m8-3-1Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  2 }

m8-3-1Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  3 }

m8-3-1Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  4 }
	
m8-3-1PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  5 }	
	
	
m8-3-1ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  6 }		
	
m8-3-1FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  7 }		
	
	
m8-3-1Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  8 }		
	
	
m8-3-1CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  9 }	
	

m8-3-1OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  10 }	

m8-3-1UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  11 }	
	
	
m8-3-1UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  12 }	
	
m8-3-1EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  13 }		
	
m8-3-1VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  14 }		
	
m8-3-1VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  15 }	
	
m8-3-1CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  16 }	
	

m8-3-1CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  17 }		

m8-3-1Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-1  18 }			
	
	
--
--	M8-3
--    	

m8-3-2Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  1 }

m8-3-2Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  2 }

m8-3-2Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  3 }

m8-3-2Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  4 }
	
m8-3-2PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  5 }	
	
	
m8-3-2ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  6 }		
	
m8-3-2FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  7 }		
	
	
m8-3-2Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  8 }		
	

m8-3-2CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  9 }	

m8-3-2OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  10 }	

m8-3-2UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  11 }	
	
	
m8-3-2UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  12 }	
	
m8-3-2EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  13 }		
	
m8-3-2VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  14 }		
	
m8-3-2VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  15 }	
	
m8-3-2CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  16 }	
	

m8-3-2CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  17 }		

m8-3-2Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-2  18 }	
	
	
--
--	M8-3
--    

m8-3-3Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  1 }

m8-3-3Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  2 }

m8-3-3Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  3 }

m8-3-3Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  4 }
	
m8-3-3PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  5 }	
	
	
m8-3-3ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  6 }		
	
m8-3-3FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  7 }		
	
	
m8-3-3Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  8 }		
	

m8-3-3CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  9 }	


m8-3-3OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  10 }	

m8-3-3UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  11 }	
	
	
m8-3-3UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  12 }	
	
m8-3-3EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  13 }		
	
m8-3-3VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  14 }		
	
m8-3-3VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  15 }	
	
m8-3-3CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  16 }	
	

m8-3-3CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  17 }	

m8-3-3Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-3  18 }	
	
--
--	M8-3
--    
	

m8-3-4Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  1 }

m8-3-4Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  2 }

m8-3-4Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  3 }

m8-3-4Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  4 }
	
m8-3-4PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  5 }	
	
	
m8-3-4ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  6 }		
	
m8-3-4FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  7 }		
	
	
m8-3-4Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  8 }		
	

m8-3-4CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  9 }	
	
m8-3-4OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  10 }	

m8-3-4UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  11 }	
	
	
m8-3-4UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  12 }	
	
m8-3-4EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  13 }		
	
m8-3-4VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  14 }		
	
m8-3-4VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  15 }	
	
m8-3-4CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  16 }	
	

m8-3-4CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  17 }		
	
m8-3-4Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-4  18 }	
		
	
--
--	M8-3
--    
	

m8-3-5Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  1 }

m8-3-5Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  2 }

m8-3-5Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  3 }

m8-3-5Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  4 }
	
m8-3-5PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  5 }	
	
	
m8-3-5ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  6 }		
	
m8-3-5FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  7 }		
	
	
m8-3-5Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  8 }	
	

m8-3-5CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  9 }	

	
m8-3-5OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  10 }	

m8-3-5UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  11 }	
	
	
m8-3-5UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  12 }	
	
m8-3-5EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  13 }		
	
m8-3-5VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  14 }		
	
m8-3-5VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  15 }	
	
m8-3-5CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  16 }	
	

m8-3-5CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  17 }	

m8-3-5Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-5  18 }	
		
	
--
--	M8-3
--    


m8-3-6Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  1 }

m8-3-6Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  2 }

m8-3-6Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  3 }

m8-3-6Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  4 }
	
m8-3-6PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  5 }	
	
	
m8-3-6ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  6 }		
	
m8-3-6FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  7 }		
	
	
m8-3-6Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  8 }	


m8-3-6CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  9 }	


m8-3-6OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  10 }	

m8-3-6UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  11 }	
	
	
m8-3-6UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  12 }	
	
m8-3-6EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  13 }		
	
m8-3-6VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  14 }		
	
m8-3-6VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  15 }	
	
m8-3-6CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  16 }	
	

m8-3-6CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  17 }	

m8-3-6Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-6  18 }	
			

--
--	M8-3
--    


m8-3-7Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  1 }

m8-3-7Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  2 }

m8-3-7Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  3 }

m8-3-7Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  4 }
	
m8-3-7PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  5 }	
	
	
m8-3-7ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  6 }		
	
m8-3-7FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  7 }		
	
	
m8-3-7Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  8 }	


m8-3-7CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  9 }	

m8-3-7OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  10 }	

m8-3-7UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  11 }	
	
	
m8-3-7UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  12 }	
	
m8-3-7EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  13 }		
	
m8-3-7VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  14 }		
	
m8-3-7VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  15 }	
	
m8-3-7CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  16 }	
	

m8-3-7CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  17 }	

m8-3-7Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-7  18 }	
		
	
--
--	M8-3
--    


m8-3-8Description OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  1 }

m8-3-8Voltage OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  2 }

m8-3-8Current OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  3 }

m8-3-8Power OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  4 }
	
m8-3-8PowerReady OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  5 }	
	
	
m8-3-8ControlInput OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  6 }		
	
m8-3-8FAIState OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  7 }		
	
	
m8-3-8Status OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  8 }	


m8-3-8CtlInputType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  9 }	

m8-3-8OutputLoadType OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  10 }	

m8-3-8UnlockOnFAIActivation OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  11 }	
	
	
m8-3-8UnlockOnAcLoss OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  12 }	
	
m8-3-8EmailAlertOnFault OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  13 }		
	
m8-3-8VoltageLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  14 }		
	
m8-3-8VoltageUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  15 }	
	
m8-3-8CurrentLowerLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  16 }	
	

m8-3-8CurrentUpperLimit OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  17 }	

m8-3-8Enable OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3-8  18 }	
	

m8-3Version OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3  9 }
    
m8-3VoltageLowerLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3  10 }

m8-3VoltageUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3  11 }

m8-3CurrentLowerLimitPercent  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3  12 }

m8-3CurrentUpperLimitPercent OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3  13 }

m8-3Measurement OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    ""
    DEFVAL { "" }
    ::= { m8-3  14 }        
    
    

--
--	MCU
--    
Time OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Time."
    DEFVAL { "" }
    ::= { netlink  1 }

SiteID OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System Site ID, it is entered by user from GUI."
    DEFVAL { "" }
    ::= { netlink  2 }

CabinetInternalTemperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System temperature on PCB board."
    DEFVAL { "" }
    ::= { netlink  3 }
    
CurrentSense1  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "HallSensor 1 Current."
    DEFVAL { "" }
    ::= { netlink  4 }
   
CurrentSense2  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "HallSensor 2 Current."
    DEFVAL { "" }
    ::= { netlink  5 }
    
ExternalTemperature OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Enviroment temperature."
    DEFVAL { "" }
    ::= { netlink  6 }
    
ADC1Reading OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    " ADC1 Voltage."
    DEFVAL { "" }
    ::= { netlink  7 }
    
ADC2Reading OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "ADC2 Voltage."
    DEFVAL { "" }
    ::= { netlink  8 }
    
Event1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Event1 status, Active or Inactive."
    DEFVAL { "" }
    ::= { netlink  10 }
    

CNTRL1 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "NL4 Fault pin output status, set as ON will output 
    low voltage, OFF will output high voltage."
    DEFVAL { "" }
    ::= { netlink  12 }

CNTRL2 OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "NL4 EN_FAI pin status, set as ON will output 
    low voltage, OFF will output high voltage."
    DEFVAL { "" }
    ::= { netlink  13 }

DeviceDetectCnt OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "System device detected."
    DEFVAL { "" }
    ::= { netlink  14 }

NextServicedue OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Service due, NO or Yes. Service date is entered by user from GUI."
    DEFVAL { "" }
    ::= { netlink  15 }
    
Status   OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "MCU  Current Status."
    DEFVAL { "" }
    ::= { netlink  16 }
    
Version  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "MCU  Version."
    DEFVAL { "" }
    ::= { netlink  17 }    


END
