IMPORTANT - Read Before Installing

*** NOTE - NetLink cannot be downgraded after installing this version.  Read the release notes carefully before installing! ***
*** Support for the MSM-200 Hardware device was discontinued at Version 9.56.  If you are using MSM-200, you must upgrade to MSM-Enterprise or use 9.53 or earlier firmware. ***

Bridge Updates: 
- If the netlink to be upgraded is below 7.15, the netlink must be upgraded to 7.15 before upgrading to 7.16 or higher.
- If the netlink to be upgraded is below 8.10, the netlink must be upgraded to 8.10 before upgrading to 8.11 or higher.
- If the netlink to be upgraded has a GREEN daughter board, the netlink must have version 9.17 or higher before upgrading to 9.18 or higher.
- If the netlink to be upgraded is below 9.79, the netlink must be upgraded to 9.79 before upgrading to 9.80 or higher.

Reboot the NetLink before installing this update.  Reboot button may be found on the Tools page of the browser interface.
Failure to reboot before installing this update may result in errors during the upgrade process.

Contact LifeSafety Power Technical Support at (888)577-2898 X2 for assistance.
